THERMOPTIM INTERACTIVE CHART.   Copyright 1998-1999   R. GICQUEL
Cycle file	April 24, 2000 6:37:24 o'clock PM CEST
lang=en
Cycle Title	Air conditioning cycle
Description	This cycle represents an air conditioning cycle
Selected gas: air, pressure (bar) : 1.01325
Number of points	5
point name	dry bulb temperature (°C)	specific humidity (kg/kg)	relative humidity	specific enthalpy (kJ/kg)	wet bulb temperature (°C)	specific volume (m3/kg)
outside air	35	0.02887	0.8	109.16173	31.81369	0.91371	
mixed air	31.7	0.02187	0.73691	87.7524	27.66855	0.89419	
cooled air	6	0.002	0.34774	11.03404	0.9088	0.79353	
supply	16	0.002	0.17887	21.08903	6.27336	0.82195	
internal air	24	0.00554	0.3	38.14015	13.70006	0.84948	
